**Art 1/G+/48**

G+ Audio only

* TCP/IP protocol "G+" digital installation.
* Casing manufactured in polished ABS white colour.
* Capacitive touch buttons with acoustic confirmation on press.
* Surface installation. Depth without strip 15mm, depth with strip 23mm.
* Includes mounting connector.
* Possibility to power it locally at 12Vdc, at 18Vdc using [D4L-G+/PoE](https://www.golmar.es/products/d4l-g-plus-poe) or [DCP/G+](https://www.golmar.es/products/dcp-g-plus) and [DCS/G+](https://www.golmar.es/products/dcs-g-plus), or at 48V standard PoE.
* Duplex audio communication.
* Privacy on audio and door open progresses.
* Do not disturb function with light indication.
* Input for doorbell apartment push button.
* Different call reception tones depending where the call is coming from.
* Volume adjustment.
* Output to auxiliary call repeater.
* Intercommunication with other monitors in the same apartment.
* Additional push button can be used to activate a second lock connected to the door panel.

**Dimensions:** 89(W) x 138(H) x 15(D) mm.

Art1/G+ user manual